XWiFi CPU

Kelly Flanagan

801-369-0033

[kelly\_flanagan@byu.edu](mailto:Kelly_flanagan@byu.edu)

Please find enclosed the BOM, circuit board, drawing, needed components, and stencil. If you have any question please call, email, or text me.

Lead based solder is fine.

The WiFi module manufacturer requires **“no clean”** solder paste and **no liquid cleaning step in the process**.

The header pins are installed from the bottom as shown in the following figure.

